foxhunt TO DO list

- fab an enclosure for the untuned RF sniffer, install and test.  RF tight is not a high priority at this time

low priority:
- redesign or at least test portable doppler (probably not a superior alternative to DF-1)
- switch fox control to a different channel, set foxes to dual vfo on the other channel for rx
- commission fox hunt logo
- determine which HTs will be for which dedicated uses
- velcro on back of 202's and gear that uses them
- program IC-2340 in truck for fox freqs
- redo DF-1 antenna connection, affix to control box
- get handheld doppler working (needs testing, would like to redesign the antenna array)
- attach offset attenuator #1 and an HT to 4 element beam (use shorter coaxes)
- get other 4 element 2m beam working, rig for truck mount
- install rf sniffer into shielded metal enclosure
- attach offset attenuator #2  to a handheld beam
- mark front of DF-1 to indicate reversed units