Oelwein repeater: 147.345+136.5
Waterloo repeater: 146.940-136.5

Checklist when hiding:

prep:
- HT battery and spare are charged
- correct data cable and controller
- enclosure and antennas
- charged and installed batteries
- fox manuals handy
- piccon reprogramming notes handy
- print several copies of a map of the area.  print both road and satellite maps
- include fox frequencies, order, and behavior on back of maps

Beacon:
	Radio: MicroFox-15
	Power: 100mW
	Preset volume: n/a
	Cable: n/a
	Piccon: n/a
notes:
	Freq: 144.100 (fox-4)
	OA/2Mhz Freq: 146.100
	Tones: random melody
	Behavior: 0:15 tx, every 0:30

Fox-3:
	Radio: Baofeng UV-3R
	Power: low
	Preset volume: 50%
	Cable: HT4P "Y"
	CleverFox
	(formerly Piccon: B, jumper ON)
program:
	A6 43 68 = "#4368" unlock code
	C1 14 30 26 25 03 # = N0ZYC morse ID
	C2 30 20 10 10 10 00 # = "3 2 1 1 1   " tone sequence
	A2 00 30 = 30 sec tx duration
	A3 01 00 = tx every 1:00
	C4 2 3 # = "tones, ID, sleep" behavior

notes:
	Freq: 146.430
	OA/2Mhz Freq: 144.430
	Tones: 3-2-1-1-1
	Behavior: 0:30 tx, every 1:00

Fox 4:
	Radio: Baofeng UV-3R
	Power: high
	Preset volume: lowest before mute
	Cable: HTBC "B"
	Piccon: A, jumper OFF
program:
	piccon: A
	A6 43 68 = "#4368" unlock code
	C1 14 30 26 25 03 # = N0ZYC morse ID
	C2 10 20 30 30 30 00 # = "1 2 3 3 3   " tone sequence
	A2 00 30 = 30 sec tx duration
	A3 01 00 = tx every 1:00
	C4 2 3 # = "tones, ID, sleep" behavior
notes:
	Freq: 144.100
	OA/2Mhz Freq: 146.100
	Tones: 1-2-3-3-3
	Behavior: 0:30 tx, every 1:00

Fox 5:
	Radio: Baofeng UV-3R
	Power: high
	Preset volume: lowest before mute
	Cable: custom
	Piccon: D, jumper OFF
program:
	A6 43 68 = "#4368" unlock code
	C1 14 30 26 25 03 # = N0ZYC morse ID
	C2 30 30 30 20 10 20 30 30 30 # = "3 3 3 2 1 2 3 3 3   " tone sequence
	A2 00 30 = 30 sec tx duration
	A3 02 00 = tx every 2:00
	C4 2 3 # = "tones, ID, sleep" behavior
notes:
	Freq: 144.525
	OA/2Mhz Freq: 146.525
	Tones: 3-3-2-1-2-3-3
	Behavior: 0:30 tx, every 2:00

Fox 6:
	Radio: Baofeng UV-3R
	Power: high
	Preset volume: lowest before mute
	Cable: custom
	Piccon: C, jumper OFF
program:
	A6 43 68 = "#4368" unlock code
	C1 14 30 26 25 03 # = N0ZYC morse ID
	C2 10 10 10 20 30 20 10 10 10 00 # = "1 1 1 2 3 2 1 1 1   " tone sequence
	A2 00 30 = 30 sec tx duration
	A3 03 00 = tx every 3:00
	C4 2 3 # = "tones, ID, sleep" behavior
notes:
	Freq: 144.820
	OA/2Mhz Freq: 146.820
	Tones: 1-1-2-3-2-1-1
	Behavior: 0:30 tx, every 3:00

VX-2R:
keypad lock: press and release Fn.  Hold Band 2 sec.

UV-3R:
keypad lock: hold Menu 2 sec (padlock icon on button)
will not power on when external power is provided over 3.2v or so

UV-5R:
- byonics piccon cable radio jack isn't deep enough and must be held
  into the jack for reliable operation
- when battery is out and running on dc power cable, the speaker
  does not work if the voltage is >= 4.8v

PICCON notes:
- had to reset a piccon that refused to adjust times

DTMF Remote Control:

1 = start transmission immediately.  begin delayed transmissions
2 = terminates play or delay timer and goes directly to next delay or play
3 = if playing, stop transmission immediately.  stop delayed transmissions
4 = DTMF lock
#nnnn = unlock using programmed code

modes 2 and 3 only work for crossband dual vfo (ability to rx on control
channel while transmitting on fox channel)

while locked, will not react to control or programming codes

feedback for Byon:
- when turned off with (DTMF-3), it should either always identify, or identify if it has not yet