DTMF Remote Control:

1 = start transmission immediately.  start behavior
2 = if transmitting, stop and begin delay.  if delaying or paused, start transmission now
	and begin timed transmissions
3 = stop transmission.  stop behavior.  requires radio to receive while transmitting
4 = lock
#nnnn = unlock using programmed code

pressing the tact switch is the same as DTMF 2

do NOT release PTT while entering individual commands.  ok to unkey between commands

(see Fox Box Notes.rtf for programming of individual foxes)

- green light will flash and turn off when battery is plugged in, and will start in a paused state
- when transmitting, green light will be on solid
- when sleeping, green light will flash slowly
- when paused, green light will be off
- when a DTMF tone is received, green light will flash rapidly for 1/2 second
- stop signal can be sent at any time.  piccon will NOT id and will go to paused state
- start signal will cause immediate start of transmit cycle. after transmit, timed transmissions will begin
- commands can be received and handled at any time.  radio must have dual VFOs and be able
  to receive on one while transmitting on the other to receive commands while transmitting.

Factory Defaults:

A1 00 00  00:00 transmit delay
A2 00 15  00:15 tone duration
A3 00 00  00:00 loop time
A4 00 00  00:00 initial delay
A5 00 00  00:00 total run time
A6 00 00  0000 unlock code
B1 88     88 tone sequence speed
B2 20     20 wpm morse code speed
B3 75     75 morse code tone
B4 00     00 Mode A flags
B5 00     00 Mode B flags
C1 16 09 03 03 15 14 27 32 29 30 #   "PICCON/2.0" morse code ID
C2 7 7 8 5 5 6 3 3 4 2 2 0 4 4 3 6 6 5 8 8 7 1 1 0 #  simple tone sequence
C4 2 3 #   undocumented default, probably tones, id, sleep

piccon reset: hold SW1 and send DTMF 0