part no	qty	description

14 PIN DIP foam:

74LS00	12	quad 2 input nand
74LS02	3	quad 2 input nor
74LS04	3	hex inverter
74LS05	2	hex inverter
74LS08	2	quad 2 input and
74LS10	3	tri 3 input nand
74LS20	9	dual 4 input nand
74LS32	3	quad 2 input or
74LS76	11	dual JK flipflop
CD4001	2	quad 2 input nor
DM7403	3	quad 2 input nand
LM324	3	quad op amp
LS193	4	4 bit counter
NE556	1	dual timer
SN7447	1	bcd to 7 segment driver, common anode
SN75188	1	quad line driver
SN75189	1	quad line receiver

8 PIN DIP foam:

LM3909	1	led lasher
LM386	1	af amp
NE555	2	timer
UA741	2	op amp

bags:

49 x 74HC145 4 bit BCD demux

38 x SN74LS124 dual VCO

10x LM358N dual op amp
10x LM3914N bar display driver
5x LM3915N bar display driver (log)
10x LM324N quad op amp
20x UDN2981 octal line driver.pdf
10x NE555 timer