Oelwein repeater: 147.345+136.5
Waterloo repeater: 146.940-136.5

Checklist when hiding:

prep:
- HT battery and spare are charged
- correct data cable and controller
- enclosure and antennas
- charged and installed batteries
- fox manuals handy
- piccon reprogramming notes handy
- print several copies of a map of the area.  print both road and satellite maps
- include fox frequencies, order, and behavior on back of maps