2235 is correct mm per rev for my 29" tires

to get into change mode, select the tach 0:00:00:00 and hold both buttons 5 sec.